create_item(" 2440AT62A0085_v1_encrypted","2440AT62A0085_v1_encrypted","X",16,-1,NULL,"Component Parameters",NULL,"%43?global %;%d:%t %# %44?0%:%31?%C%:_net%c%;%;%e %b%r%8?%29?%:%30?%p %:%k%?[%1i]%;=%p %;%;%;%e%e","2440AT62A0085_v1_encrypted","%t%b%r%38?%:\n%30?%s%:%k%?[%1i]%;=%s%;%;%e%e%;","",0,NULL,0,create_parm("CustomComponentLayer","Layer in the substrate corresponding to Z=0 in the 3D Component",2624,"ckt_pad_layer",-1,prm("layer_text_form","cond:drawing"))
,create_parm("CustomComponentOnTop","Alignment of Z=0 in the 3D Component with top/bottom of the layer",2656,"boolean",-1,prm("boolean_yes"))
,create_parm("CustomComponentRotateX","Rotate the 3D Component around X-axis",68160,"StdFormSet",7,prm("StdForm","0"))
,create_parm("CustomComponentRotateY","Rotate the 3D Component around Y-axis",68160,"StdFormSet",7,prm("StdForm","0"))
,create_parm("CustomComponentMirrorZ","Mirror 3D Component about XY-plane",2656,"boolean",-1,prm("boolean_no"))
,create_parm("CustomComponentOffsetZ","Additional offset in Z-direction of the 3D Component",68160,"StdFormSet",5,prm("StdForm","0"))
,create_parm("Airbox","",67584,"StdFormSet",5,prm("StdForm","200 mm"))
,create_parm("Ground","",67584,"StdFormSet",5,prm("StdForm","50 mm"))
,create_parm("SilverX","",67584,"StdFormSet",5,prm("StdForm","8 mm"))
,create_parm("CUT","",67584,"StdFormSet",5,prm("StdForm","1.3 mm"))
,create_parm("DX","",67584,"StdFormSet",5,prm("StdForm","3.6 mm"))
,create_parm("PatchH","",67584,"StdFormSet",5,prm("StdForm","4 mm"))
,create_parm("AirboxH","",67584,"StdFormSet",5,prm("StdForm","200 mm"))
,create_parm("PatchW","",67584,"StdFormSet",5,prm("StdForm","12 mm"))
,create_parm("FeedY","",67584,"StdFormSet",5,prm("StdForm","1.2 mm"))
,create_parm("SilverY","",67584,"StdFormSet",5,prm("StdForm","7.68 mm"))
,create_parm("feedtop","",67584,"StdFormSet",5,prm("StdForm","1.2 mm"))
,create_parm("sidebottom","",67584,"StdFormSet",5,prm("StdForm","2 mm"))
,create_parm("sidetop","",67584,"StdFormSet",5,prm("StdForm","2 mm"))
,create_parm("FeedX","",67584,"StdFormSet",5,prm("StdForm","2 mm"))
,create_parm("sideH","",67584,"StdFormSet",5,prm("StdForm","4 mm"))
,create_parm("MoveY","",67584,"StdFormSet",5,prm("StdForm","0 mm"))
,create_parm("MOVE","",67584,"StdFormSet",5,prm("StdForm","0 mm"))
,create_parm("DY","",67584,"StdFormSet",5,prm("StdForm","2 mm"))
,create_parm("PatchL","",67584,"StdFormSet",5,prm("StdForm","12 mm"))
,create_parm("maxFreq","Maximum frequency of interest for the project.",68096,"StdFormSet",0,prm("StdForm","4 GHz"))
,create_parm("minFreq","Minimum frequency of interest for the project.",68096,"StdFormSet",0,prm("StdForm","1 GHz"))
);
