<!DOCTYPE Materials>
<Materials>
    <Conductors>
        <Conductor parmtype="1" mur_imag="" mur_real="1" thermal_conductivity_in_z="" imag="" tc1="" real="5.8e7 Siemens/m" tc2="" thermal_conductivity="401" heat_capacity="2.49E+06" electron_path="" tnom="" name="Copper"/>
    </Conductors>
    <Dielectrics>
        <Dielectric mur_imag="" mur_real="1" highfreq="1 THz" thermal_conductivity_in_z="" loss_type="1" lowfreq="1 KHz" thermal_conductivity="25.25" er_imag="" heat_capacity="1.73E+06" electron_path="" er_loss="" valuefreq="1 GHz" name="Alumina" er_real="9.6"/>
        <Dielectric mur_imag="" mur_real="1" highfreq="1 THz" thermal_conductivity_in_z="" loss_type="1" lowfreq="1 KHz" thermal_conductivity="" er_imag="" heat_capacity="" electron_path="" er_loss="" valuefreq="1 GHz" name="Dielectric_1" er_real="1"/>
        <Dielectric mur_imag="" mur_real="1" highfreq="1 THz" thermal_conductivity_in_z="" loss_type="1" lowfreq="1 KHz" thermal_conductivity="" er_imag="" heat_capacity="" electron_path="" er_loss="0.01" valuefreq="1 GHz" name="FR_4" er_real="4.6"/>
    </Dielectrics>
    <Semiconductors/>
    <Superconductors/>
    <roughness/>
</Materials>
