TECHFORMAT=V2

UNITS
  DISTANCE=METRE
  CONDUCTIVITY=SIEMENS/M
  RESISTIVITY=OHM.CM
  RESISTANCE=OHM/SQ
  PERMITTIVITY=RELATIVETOVACUUM
  PERMEABILITY=RELATIVETOVACUUM
  FREQUENCY=HZ
  TEMPERATURE=CELSIUS
END_UNITS

BEGIN_MATERIAL
  MATERIAL Copper CONDUCTIVITY=5.8e7 IMAG_CONDUCTIVITY=0 PERMEABILITY=1
  MATERIAL FR_4 PERMITTIVITY=4.6 LOSSTANGENT=0.01 PERMEABILITY=1 DJORDJEVIC LOWFREQ=1000 VALUEFREQ=1000000000 HIGHFREQ=1000000000000
END_MATERIAL

BEGIN_OPERATION
  OPERATION OperationSHEET SHEET
  OPERATION OperationThickness_Bottom_Metal INTRUDE=3.556e-05 DOWN
  OPERATION OperationThickness_Top_Metal INTRUDE=3.556e-05 UP
  OPERATION OperationBoundaryOutline BOUNDARYOUTLINE
  OPERATION OperationDRILL DRILL
  OPERATION OperationTSV_VIA DRILL
  OPERATION OperationTSV_Hole DRILL
END_OPERATION

BEGIN_MASK
  MASK 0 Name=Bottom_Metal PRECEDENCE=0 COLOR="ff0000" MATERIAL=Copper OPERATION=OperationThickness_Bottom_Metal MASK_PROPERTIES = { "TopTechnologyMaskName=Bottom-Metal", "OriginalName=Bottom-Metal" }
  MASK 1 Name=Top_Metal PRECEDENCE=1 COLOR="ffff00" MATERIAL=Copper OPERATION=OperationThickness_Top_Metal MASK_PROPERTIES = { "TopTechnologyMaskName=Top-Metal", "OriginalName=Top-Metal" }
  MASK 2 Name=VIA PRECEDENCE=0 COLOR="00c000" MATERIAL=Copper OPERATION=OperationDRILL
  MASK 3 Name=Hole PRECEDENCE=0 COLOR="00ffff" MATERIAL=Copper OPERATION=OperationDRILL
  MASK 4 Name=CUT COLOR="0000ff" OPERATION=OperationBoundaryOutline
END_MASK

BEGIN_STACK
  Name=EVB_mm
  PRECEDENCE=0
  TOP OPEN MASK={CUT} MATERIAL=AIR
  INTERFACE Name=__Interface1      MASK={Top_Metal CUT}
  LAYER     Name=__SubstrateLayer1 MASK={VIA Hole CUT} HEIGHT=0.0008 MATERIAL=FR_4
  INTERFACE Name=__Interface0      MASK={Bottom_Metal CUT}
  BOTTOM OPEN MASK={CUT} MATERIAL=AIR
END_STACK

