; Top Design: "EVB_mm_lib:Ant_Test:schematic"
; Netlisted using Hierarchy Policy: "Standard"

Options ResourceUsage=yes UseNutmegFormat=no EnableOptim=no TopDesignName="EVB_mm_lib:Ant_Test:schematic" DcopOutputNodeVoltages=yes DcopOutputPinCurrents=yes DcopOutputAllSweepPoints=no DcopOutputDcopType=0
; Library Name: EVB_mm_lib
; Cell Name: 0900AD47A2450-EB1SMA
; View Name: schematic_0900AD47A2450
define "0900AD47A2450-EB1SMA" ( P1  P2 ) 
;parameters 
Short:Short  0 Ref Mode=0 SaveCurrent=no 
#ifndef inc_EVB__mm__lib_3a0900AD47A2450_2dEB1SMA_3aschematic__0900AD47A2450__D_3a_5cProjects_5cADS_5cJohansonAntenna_5c__3DAnt__test__v2__wrk_2f_5cdata_2f0900AD47A2450__outplan_2edef
#define inc_EVB__mm__lib_3a0900AD47A2450_2dEB1SMA_3aschematic__0900AD47A2450__D_3a_5cProjects_5cADS_5cJohansonAntenna_5c__3DAnt__test__v2__wrk_2f_5cdata_2f0900AD47A2450__outplan_2edef 1
#include "D:\Projects\ADS\JohansonAntenna\_3DAnt_test_v2_wrk\data\0900AD47A2450_outplan.def"
#endif
#uselib "ckt" , "SnP"
SnP:"0900AD47A2450"  P1 P2 "C1_P1_C1\.P1_C1_P2_C1\.P1" "L1_P1_C1\.P1_L1_P2_P2" "L2_P1_L2\.P1_L2_P2_P1" "C2_P1_P1_C2_P2_C1\.P1" "L3_P1_P1_L3_P2_C1\.P1" Ref NumPorts=7 File="D:\Projects\ADS\JohansonAntenna\_3DAnt_test_v2_wrk\data\0900AD47A2450-EB1SMA_rfpro_0900AD47A2450.sio" Type="smatrixio" InterpMode="linear" InterpDom="" ExtrapMode="constant" Temp=27.0 CheckPassivity=0 

L_5p1nH_R5=0
L_5p1nH_L5=5.1e-09 tune{ 2.55e-09 to 7.65e-09 by 5.1e-10 }
L_5p1nH_C5=0
#uselib "ckt" , "SRLC"
SRLC:C2  "C2_P1_P1_C2_P2_C1\.P1" Ref R=C_8p2pF_R4 L=C_8p2pF_L4 C=C_8p2pF_C4 

C_8p2pF_R4=0
C_8p2pF_L4=0
C_8p2pF_C4=9.4e-12 tune{ 4.7e-12 to 1.41e-11 by 9.4e-13 }
#uselib "ckt" , "SRL"
SRL:L2  "L2_P1_L2\.P1_L2_P2_P1" Ref R=L_12nH_R3 L=L_12nH_L3 

L_12nH_R3=0
L_12nH_L3=1.275e-08
L_12nH_C3=0
#uselib "ckt" , "SRL"
SRL:L1  "L1_P1_C1\.P1_L1_P2_P2" Ref R=L_2p7nH_R2 L=L_2p7nH_L2 

L_2p7nH_R2=0
L_2p7nH_L2=5.94e-09
L_2p7nH_C2=0
#uselib "ckt" , "SRLC"
SRLC:C1  "C1_P1_C1\.P1_C1_P2_C1\.P1" Ref R=C_1p0pF_R1 L=C_1p0pF_L1 C=C_1p0pF_C1 

C_1p0pF_R1=0
C_1p0pF_L1=0
C_1p0pF_C1=0.732e-12
end "0900AD47A2450-EB1SMA"

S_Param:SP1 CalcS=yes CalcY=no CalcZ=no GroupDelayAperture=1e-4 FreqConversion=no FreqConversionPort=1 StatusLevel=2 CalcNoise=no SortNoise=0 BandwidthForNoise=1.0 Hz DevOpPtLevel=0 SPSS_WSP=yes \
SweepVar="freq" SweepPlan="SP1_stim" OutputPlan="SP1_Output" 

SweepPlan: SP1_stim Start=0.5 GHz Stop=3 GHz Step=0.005 GHz 

OutputPlan:SP1_Output \
      Type="Output" \
      UseEquationNestLevel=yes \
      EquationNestLevel=2 \
      UseSavedEquationNestLevel=yes \
      SavedEquationNestLevel=2

#load "python","LinearCollapse"
Component Module="LinearCollapse" Type="ModelExtractor" NetworkRepresentation=2
Port:TermG1  N__0 0 Num=1 Z=50 Ohm Noise=yes 
"0900AD47A2450-EB1SMA":X4  N__0 N__1 
Port:TermG2  N__1 0 Num=2 Z=50 Ohm Noise=yes 
